**ANNEXURE - II**

**APPROVED SPECIFICATION FOR LINE BUS**

1. Line Bus should be of modern and elegantly designed ordinary bus.
2. Wheel base should not exceed 2700 mm
3. Flooring should be of flat type
4. The design of passenger seats should be simple (not bucket type).
5. Roof top luggage carrier with suitable size should be provided along with ladder.
6. Emergency exit should be provided for safety measures.
7. Name, full address and contact No. of the owner should be clearly inscribed inside and outside near the passengers’ door.
8. Colour of the bus should be prescribed by the STA from time to time.
9. The word AIZAWL CITY LINE BUS should be inscribed clearly on both sides of the wall.
10. The seating capacity of line bus should not exceed 17+1(D)
11. The following accessories should be provided in the bus:
12. Rear view mirror - 2 nos
13. Inside rear view mirror - 1 no
14. First aid box - 1 no
15. Fire extinguisher (1 Kg capacity) - 1 no
16. Tools - 1 set

(Vide STA Meeting Dt. 13th December, 2016.)